**Release Notes Drivers Pack 3.74**

**Driver package of IP devices for Axxon One software**

**September 5, 2022. Release notes**

For information about the Drivers Pack, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

**98 new IP devices are integrated**

**IP-cameras:**

ABUS IPCB34511A

ABUS IPCB34511B

ABUS IPCB38511A

ABUS IPCB38511B

ABUS IPCB44511A

ABUS IPCB44511B

ABUS IPCB44611A

ABUS IPCB44611B

ABUS IPCB54511A

ABUS IPCB54511B

ABUS IPCB54611B

ABUS IPCS34511A

ABUS IPCS34511B

ABUS IPCS54511A

ABUS IPCS54511B

ABUS IPCS64511A

ABUS IPCS64511B

ABUS IPCB68621

Axis M1137

Axis Q3517

Axis Q8414-LVS

Axis Q8685-LE

Axis P3247-LVE

Beward SV3210R2

Beward SV3210RCB

Beward SV3210RZ2

Beward SV3217DB

Beward SV3217DBS

Beward SV3217DBZ

Beward SV3217DM

Beward SV3217M

Beward SV3217RZ2

Beward SV3217RBZ

Beward SV3217RZX

CP PLUS CP-VNC-T41ZR5C-MD

CP PLUS CP-VNC-T41ZR3-MD

CP PLUS UNC-TC51ZL6-VMDS

Grundig GD-CI-AP6637T

Hanwha Techwin QND-6082R

Hanwha Techwin QNV-6082R

Hikvision DS-2CD2043G2-IU

Hikvision DS-2CD2443G2-I

Hikvision DS-2CD2543G2-IS

Hikvision DS-2CD2546G2-IS

Hikvision DS-2CD3626G2T-IZS

Hikvision DS-2CD3726G2T-IZS

Hikvision DS-2CD3D26G2T-IZHS

Hikvision DS-2CD3D26G2T-IZHSY

HiWatch DS-I214(B)

HiWatch DS-I450M

HiWatch IPC-C042-G0/W

IDIS DC-C4212RX

LTV LTV-5CNB20-F28

LTV LTV-5CNB20-F36

LTV LTV-5CND20-F28

LTV LTV-5CND20-F36

LTV LTV-5CNB40-F36

LTV LTV-5CND40-F28

LTV LTV-5CND40-F36

LTV LTV-5CNТ40-F28

LTV LTV-5CNТ40-F36

RVi RVi-2NCT2170 (2.8)

RVi RVi-2NCT2179 (2.8-12)

RVi RVi-2NCD2178 (2.8)

RVi RVi-2NCE2379 (2.8-12)

RVi RVi-2NCT5350 (2.8)

RVi RVi-2NCD5358 (2.8)

RVi RVi-2NCE5359 (2.8-12)

RVi RVi-2NCT8340 (2.8)

RVi RVi-2NCD8348 (2.8)

RVi RVi-2NCE8349 (2.8-12)

SERVICE TELEMATIKA ST-MetaCam-BC5241EP-Z12E

**NVR:**

BestDVR BestDVR-1604A-S

Hikvision DS-7608NI-I2

Hikvision DS-7608NI-I2/8P

Hikvision DS-7808NI-I2/8P

VIVOTEK ND9213P

VIVOTEK ND9323P

**DVR:**

Hikvision DS-7304HUHI-K4

Hikvision DS-7308HUHI-K4

Hikvision DS-7324HQHI-K4

Hikvision DS-8108HUHI-K8

Hikvision DS-8124HQHI-K8

Hikvision DS-8132HQHI-K8

Hikvision DS-9008HUHI-K8

Hikvision iDS-7216HQHI-M1/S

**HDVR:**

Hikvision DS-7104HUHI-K1

Hikvision DS-7204HUHI-K1/P

Hikvision DS-7104HQHI-K1

Hikvision DS-7204HQHI-K1/P

Hikvision DS-7204HUHI-K2

Hikvision DS-7208HQHI-K2

Hikvision DS-7208HQHI-K1

Hikvision DS-7216HGHI-K1

Hikvision DS-7216HGHI-K2

**I/O Module**

MOXA ioLogik E1214

**Security Radar**

Axis D2110-VE

**Network speaker**

Axis C1410

**New features and improvements**

• ONVIF, FFMPG, RTSP drivers have been improved;

• Generic drivers Axis Generic, Hanwha Techwin Generic and Bosch Generic have been improved;

• Added support for additional features of 135 devices from the following vendors: ABUS, Axis, Beward, Bosch, Dahua, EVS, Grundig, Hikvision, HiWatch, Huawei, IDIS, LTV, Milesight, Naziraty, Redline, RVi, Service Telematika, Sony, Tyco, Uniview, VIVOTEK

**Documentation and installation**

Operation of IP devices differs for various AxxonSoft products. Please refer to the [table](https://docs.axxonsoft.com/confluence/display/DDP/En) to check what features and firmware versions of integrated IP devices are supported.

To download the installer for Drivers Pack 3.74, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

To install Drivers Pack, close the VMS, run the installation file IPDriverPack.msi, complete the installation, and restart the VMS.

If Drivers Pack 3.2.0 or an earlier version is installed, first go to "Windows Control Panel" → "Add/Remove Programs" and uninstall it.

**Drivers Pack 3.74** is recommended to be used with **Axxon One 1.0.4**