**Release Notes Drivers Pack 3.76**

**Driver package of IP devices for Axxon PSIM and Axxon One softwares**

**April 12, 2023. Release notes**

For information about the Drivers Pack, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

**115 new IP devices are integrated**

**IP-cameras:**

Axis M3068-P

Axis M3086-V

Axis M3116-LVE

Axis M5075-G

Axis P1455-LE-3

Axis P1455-LE-3

Axis P3247-LV / P3247-LVE

Axis P3267-LV

Axis P3267-LV

Axis P3268-LVE

Axis P3375-LV

Axis P5414-E

Axis Q1615 Mk III

Axis Q1656-LE

Axis Q1659

Axis Q1715

Axis Q3536-LVE

Axis Q6010-E

Axis Q6078-E

Axis Q6100-E

Axis Q6215-LE

Axis V5915

Axis V5915

Axis V5938

Bosch Dinion IP NWC-xxxx series

Dahua DH-IPC-EB5531

Dahua DH-IPC-HDBW2431F-AS-S2

Dahua DH-IPC-HDBW2431R-ZAS-S2

Dahua DH-IPC-HDBW2431R-ZS-S2

Dahua DH-IPC-HDBW3441E-AS

Dahua DH-IPC-HDBW3441E-S

Dahua DH-IPC-HDBW3441F-AS-M

Dahua DH-IPC-HDBW5241F-M12-SA

Dahua DH-IPC-HDBW5241F-M-SA

Dahua DH-IPC-HDBW5541E-ZE-OPAT

Dahua DH-IPC-HDBW5541R-ASE-OPAT

Dahua DH-IPC-HDW3441TM-AS

Dahua DH-IPC-HDW3441T-ZAS

Dahua DH-IPC-HFW2231TP-AS-0360B-S2-QH

Dahua DH-IPC-HFW3441E-AS

Dahua DH-IPC-HFW3441E-SA

Dahua DH-IPC-HFW3441M-AS-I2

Dahua DH-IPC-HFW3441T-ZAS

Dahua DH-IPC-HFW3441T-ZS

Dahua DH-IPC-HFW5541E-ZE-OPAT

Dahua DH-IPC-HFW5541T-ASE-OPAT

Dahua DH-IPC-HFW7442HP-Z-S2

Dahua DH-SD1A404XB-GN

Dahua DH-SD1A404XB-GN-W

GIT GIT-CDM25AI

GIT GIT-CPDM223AI

GIT GIT-CPWM212AI

GIT GIT-CWM25AI

GIT-CSM236AI

GIT-CWM25AIL

Grundig GD-CI-AC5617E

Grundig GD-CI-BT4537TH

Hanwha Techwin XNO-8082R

Hikvision DS-2CD2345G0P-I

HiWatch IPC-B042C-G2/UL

HiWatch IPC-B522-G2/4I

HiWatch IPC-B542-G2/4I

HiWatch IPC-B642-G2/ZS

HiWatch IPC-D042C-G2/SU

HiWatch IPC-D082-G2/U

HiWatch IPC-D622-G2/ZS

HiWatch IPC-D642-G2/ZS

IDIS DC-S3883HRX

LTV LTV-3CNSD20-Z33-F

LTV LTV-GICDM4-T600-M1

LTV CNU-220 64

LTV CNU-840 58

LTV LTV CNE-642 58

LTV LTV CNU-220 62

LTV LTV LTV-3CNSD40-Z33

LTV LTV-2CNB40-M0722

LTV LTV-2CNB40-M2812

LTV LTV-3CNB20-M0550-F

LTV LTV-3CNB20-M2812-HB

LTV LTV-3CNB40-M2812-F

LTV LTV-3CNB40-M2812-HB

LTV LTV-3CND40-M2812-F

LTV LTV-CNE-880 58

LTV LTV-GICDM4-E600-M1

LTV LTV-GICDM4-E600-M2

LTV LTV-GICDM4-T700-M1

Milesight MS-C5383-PB/V

Milesight MS-C8152-PC

Milesight MS-C8162-FIPC

Milesight MS-C8162-FPC

Milesight MS-C8163-PC

Milesight MS-C8164-FIPC

Milesight MS-C8164-FPC

Milesight MS-C8172-FIPC

Milesight MS-C8172-FPC

Milesight MS-C8173-PC

Milesight MS-C8252-PC

Milesight MS-C8262-FIPC

Milesight MS-C8262-FPC

Milesight MS-C8266-X4PC

Milesight MS-C8272-FIPC

Milesight MS-C8272-FPC

NIC Tehnologii 2BD-27135

NIC Tehnologii 5BD-27135

Panasonic WV-S1536L

Panasonic WV-S2136

Panasonic WV-S2136L

Vivotek FE9391-EHV-v2

**Thermal Imaging Camera**

Axis Q1952-E

**NVR**

Dahua DHI-NVR4216-I

Hanwha Techwin XRN-6410B2

Hanwha Techwin XRN-6410RB2

VidoNet VTN-464

**Intercom**

Dahua DH-VTA2302A

**Generic driver**

DSSL generic

**New features and improvements**

• ONVIF, FFMPEG, RTSP, Universal drivers have been improved

• Generic drivers Axis Generic, Hanwha Techwin Generic and Bosch Generic have been improved;

• Added support for additional features of 153 devices from the following vendors: ABUS, Axis, Beward, Bosch, Commbox, CP Plus, Dahua, Fine, GIT, Grundig, Hanwha Techwin, Hikvision, Huawei, IDIS, LTV, Milesight, Mobotix, NIC Tehnologii, Pelco, SERVICE TELEMATIKA, RVi, Sunell, TVT, VidoNet, Vigilate, VIVOTEK

**Documentation and installation**

Operation of IP devices differs for various AxxonSoft products. Please refer to the [table](https://docs.axxonsoft.com/confluence/display/DDP/En) to check what features and firmware versions of integrated IP devices are supported.

To download the installer for Drivers Pack 3.76, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

To install Drivers Pack, close the VMS, run the installation file IPDriverPack.msi, complete the installation, and restart the VMS.

If Drivers Pack 3.2.0 or an earlier version is installed, first go to "Windows Control Panel" → "Add/Remove Programs" and uninstall it.

**Drivers Pack 3.76** is recommended to be used with **Axxon PSIM 1.0.0.48** and **Axxon One 1.0.4.65**