**Release Notes Drivers Pack 3.79**

**Driver package of IP devices for Axxon PSIM and Axxon One softwares**

**January 23, 2024. Release notes**

For information about the Drivers Pack, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

**Integrated IP devices**

Axis P3265-LVE

Axis P3267-LVE

Dahua DH-IPC-HDBW5442EP-ZE

Dahua DH-IPC-HDW3249H-AS-PV

Dahua DH-IPC-HDW5442TMN-AS-LED

Dahua DH-IPC-HF5442F-ZE

Dahua DH-IPC-HFW3249T1-AS-PV

Dahua DH-IPC-HFW3249T1N-AS-PV

Dahua DH-IPC-HFW5442EP-ZE

Dahua DH-IPC-HFW5442H-ZHE

Dahua DH-ITC431-RW1F-IRL8

Dahua DH-NVR4216-16P-4KS2/L

Grundig GD-RT-BC3008N

Hikvision DS-2CD2743G2-IZS

Hikvision DS-2CD3B46G2T-IZHS

Hikvision DS-7316HQHI-SH(B)

Hikvision DS-7608NI-E2/8P/A

Hikvision iDS-9032HUHI-M8/S

IDIS DC-Y6516WRX-A

Inaxsys Legend INLGBO4KIRWA

Inaxsys Legend INLGBO5IRWA

Inaxsys STORM INS161624KN

Inaxsys STORM INSAITO4NCF

Inaxsys STORM INSBO2IRF-PK6

Inaxsys STORM INSBO2IRWA-PK6

Inaxsys STORM INSDO2IRWA-PK6

Inaxsys STORM INSTO2IRF

Inaxsys STORM INSTO2IRF-PK6

Inaxsys STORM INSTO4IRWF

Inaxsys STORM INSTO4IRWFB

Uniview IPC324LR3-VSPF28-D

Uniview IPC8542ER5-DUP

WatchNET MPIX1-IPC154

WatchNET MPIX-40BILR-LPR

WatchNET MPIX-40LEDT-NPC28AI

**New features and improvements**

• ONVIF, FFMPEG, RTSP, Universal drivers have been improved;

• Axis Generic, Hanwha Techwin Generic, Bosch Generic, Dahua Generic, Panasonic Generic have been improved;

• Added support for additional features of 105 devices from the following vendors: Axis, Bosch, Dahua, eVidence, Hikvision, Uniview, WatchNET

**Documentation and installation**

Operation of IP devices differs for various AxxonSoft products. Please refer to the [table](https://docs.axxonsoft.com/confluence/display/DDP/En) to check what features and firmware versions of integrated IP devices are supported.

To download the installer for Drivers Pack 3.79, refer [here](https://www.axxonsoft.com/support/downloads/drivers-pack).

To install Drivers Pack, close the VMS, run the installation file IPDriverPack.msi\ IPDriverPack.deb, complete the installation, and restart the VMS.

If Drivers Pack 3.2.0 or an earlier version is installed, first go to "Windows Control Panel" → "Add/Remove Programs" and uninstall it.

**Drivers Pack 3.79** is recommended to be used with **Axxon PSIM 1.0.1.172** and **Axxon One 2.0.0**